

**8. You have a Cisco switch and a VoIP phone that needs to be placed in a voice VLAN (VLAN 20). The data for the PC should remain in a separate VLAN (VLAN 10). Configure the switch port to support both voice and data traffic.**


**Setting Up:**


****

**Configuring the switch:**

****

**Switch Support both Voice and data traffic:**

****

****